For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector from the cruise release switch.
2. Complete the following in order to remove the cruise release switch from the brake pedal bracket:

2.1. | Rotate the switch counter clockwise.

2.2. | Pull the switch from the retainer.

2.3. | Push the locking tabs inward to release the retainer.

### Installation Procedure

1. Connect the electrical connector to the cruise release switch.
2. Adjust the cruise release switch. Refer to Cruise Release Switch Adjustment .