For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Disconnect the evaporative emission (EVAP) canister vent solenoid valve electrical connector (1).
3. Disconnect the fuel fill pipe vapor line quick connect (1) from the EVAP canister. Refer to Plastic Collar Quick Connect Fitting Service .
4. Disconnect the EVAP canister vent solenoid valve quick connect from the EVAP canister. Refer to Plastic Collar Quick Connect Fitting Service .
5. Disengage the bracket retaining tab and remove the EVAP canister vent solenoid valve (1).

### Installation Procedure

1. Engage the bracket retaining tab and install the EVAP canister vent solenoid valve (1).
2. Connect the EVAP canister vent solenoid valve quick connect to the EVAP canister. Refer to Plastic Collar Quick Connect Fitting Service .
3. Connect the fuel fill pipe vapor line quick connect (1) to the EVAP canister. Refer to Plastic Collar Quick Connect Fitting Service .
4. Connect the EVAP canister vent solenoid valve electrical connector (1).
5. Lower the vehicle.