For 1990-2009 cars

### Removal Procedure

Note: The mode cam can be accessed from the driver side floor near the accellorator peddle.

1. Remove the mode control cable (4) from the retaining clip (3).
2. Remove the mode control cable (4) from the mode cam (2).
3. Remove the screw (1) from the mode cam.
4. Remove the mode cam.

### Installation Procedure

1. Install the mode cable (4).
2. Make certain that the cable is properly seated in the notch in the HVAC module.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the mode cam screw. Tighten the screw to 2 N·m (18 lb in).
4. Install the mode control cable (4) to the mode cam (2).
5. Install the mode control cable (4) to the retaining clip (3).