For 1990-2009 cars

### Removal Procedure

1. Use a trim tool to remove the head (1) of the push-pin, right and left side.
2. Use a trim tool to remove the base (1) of the push-pin, right and left side.
3. Remove the lower center instrument panel (I/P) trim from the vehicle.

### Installation Procedure

1. Install the lower center I/P trim to the vehicle.
2. Install the base (1) of the push-pin, right and left side.
3. Install the head (1) of the push-pin, right and left side.