For 1990-2009 cars

## Console Replacement Small W/ Manual Transmission

### Removal Procedure

1. Release the retaining strips on the shift lever boot.
2. Remove the inside rear seat track bolts on both front seats.
3. Lift up on the console to release the 4 retainers.
4. Remove the console from the vehicle.

### Installation Procedure

1. Position the console to the floor panel.
2. Ensure the retainers are indexed to the corresponding holes in the floor panel.
3. Push downward on the console seating the retainers.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the seat track bolts on both front seats.

Tighten
Tighten the bolts to 53 N·m (39 lb ft).

5. Attach the retaining strips on the shift lever bezel.

## Console Replacement Large w/Manual or Auto Transmission

### Removal Procedure

1. For regular cab vehicles, remove the passenger front bucket seat. Refer to Front Seat Replacement - Bucket .
2. For regular, extended and crew cab vehicles, remove the front bucket seat fasteners retaining the floor console to the floor. Refer to Front Seat Replacement - Bucket .
3. If the vehicle is equipped with a floor mounted shift lever, remove the shift lever bezel and boot.
4. Lift upward on the front and middle section of the console to release the retainers.
5. Remove the console from the vehicle.

### Installation Procedure

1. Position the console to the floor panel.
2. Ensure the retainers are indexed to the corresponding holes in the floor panel.

Important: Ensure the console bracket is positioned under the seat frame.

3. Push downward on the console to seat the retainers.
4. If the vehicle is equipped with a floor mounted shift lever, install the shift lever bezel and boot.
5. Install the console bolts and if necessary, install the front bucket seat . Refer to Front Seat Replacement - Bucket .