For 1990-2009 cars

### Removal Procedure

1. Remove the intake manifold cover. Refer to Upper Intake Manifold Sight Shield Replacement.
2. Remove the spark plug wire from the ignition coil.
3. Disconnect the ignition coil electrical connector.
4. Remove the ignition coil bolts.
5. Remove the ignition coil.

### Installation Procedure

1. Install the ignition coil.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the ignition coil bolts.

Tighten
Tighten the bolts to 8 N·m (71 lb in).

3. Connect the ignition coil electrical connector.
4. Connect the spark plug wire to the ignition coil.
5. Install the intake manifold cover. Refer to Upper Intake Manifold Sight Shield Replacement.