For 1990-2009 cars

#### Tools Required

• | J 21426 Rear Seal Installer

• | J 39440 Extension Housing Seal Installer or equivalent

1. Using the J 21426 , install an output shaft sleeve (690) and an output shaft seal (691).

Do not push the sleeve past the machined surface on the output shaft.

2. Install the case extension to case seal (30) and the case extension (31).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the case extension to case bolts (32).

Tighten
Tighten the bolts to 45 N·m (33 lb ft).

4. Inspect the transmission speed sensor for the following conditions:

• | Cracks

• | Nicks

• | Damage

5. Install a new O-ring seal (37) on the internal transmission speed sensor (36).
6. Install the internal transmission speed sensor (36).
7. Install the speed sensor retaining bolt (35).

Tighten
Tighten the bolt to 12 N·m (9 lb ft).

Important: If installing a slip yoke (booted) type seal (34), position drain hole (1) toward the bottom of transmission within area shown.

8. Using the J 21426 and J 39440 or equivalent, install the case extension oil seal assembly (34) (model dependent).