For 1990-2009 cars

### Removal Procedure

1. Remove the oil filter. Refer to Engine Oil and Oil Filter Replacement .
2. Remove the oil filter adapter from the engine block.

### Installation Procedure

Notice: Refer to Component Fastener Tightening Notice in the Preface section.

1. Install the oil filter adapter into the engine block.

Tighten
Tighten the adapter to 50 N·m (37 lb ft).

2. Install the oil filter. Refer to Engine Oil and Oil Filter Replacement .