For 1990-2009 cars

### Removal Procedure

1. Open the tailgate.
2. Remove the screws (1) from the tail lamp assembly.
3. Remove the lamp assembly.
4. Remove the tail lamp and backup lamp sockets, depressing the locking tab and rotating counterclockwise.
5. Remove the bulbs from the backup lamp sockets.

### Installation Procedure

1. Install the bulbs to the backup lamp sockets.
2. Install the backup lamp rotating clockwise until the locking tab is fully seated.
3. Press the tail lamp to the rear body panel until fully seated.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the tail lamp screws (1) to the tail lamp.

Tighten
Tighten the tail lamp screws (1) to 3 N·m (26 lb in).

5. Close the tailgate.