For 1990-2009 cars

### Removal Procedure

1. Remove the steering column tilt head housing. Refer to Steering Column Tilt Head Housing Replacement .
2. Remove the steering shaft upper bearing from the steering column tilt head housing.

### Installation Procedure

1. Install the steering shaft upper bearing into the steering column tilt head housing.
2. Install the steering column tilt head housing. Refer to Steering Column Tilt Head Housing Replacement .