For 1990-2009 cars

### Removal Procedure

1. Open the door.
2. Remove the screw securing the seat back release knob to the seat.
3. Remove the seat back release knob.

### Installation Procedure

1. Position the seat back release knob onto the seat assembly.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the screw securing the seat back release knob to the seat.

Tighten
Tighten the front seat back release knob screw to 1.5 N·m (13 lb in).