For 1990-2009 cars

### Removal Procedure

1. Remove the floor console. Refer to Console Replacement .
2. Roll the carpeting back to expose the rear floor air ducts.
3. Remove the rear floor ducts from the floor studs.
4. Remove the rear floor duct.

### Installation Procedure

1. Install the rear floor air duct.
2. Install the rear floor ducts from the floor studs.
3. Position the carpeting back into place.
4. Install the floor console. Refer to Console Replacement .