For 1990-2009 cars

### Removal Procedure

1. Open the rear seat belt upper guide shoulder bolt trim cover.
2. Remove the rear seat belt upper guide shoulder bolt.
3. Remove the knob from the rear seat belt shoulder adjuster (1).
4. Remove the body rear corner upper trim panel (2). Refer to Body Side Upper Trim Panel Replacement .
5. Remove the 2 bolts securing the adjuster to the vehicle.
6. Remove the rear seat belt shoulder adjuster from the vehicle.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the 2 bolts securing the rear seat belt shoulder adjuster (1) to the vehicle.

Tighten
Tighten the rear seat belt shoulder adjuster bolts to 52.5 N·m (39 lb ft).

2. Install the body rear corner upper trim panel (2). Refer to Body Side Upper Trim Panel Replacement .
3. Install the knob on the rear seat belt shoulder adjuster (1).
4. Install the rear seat belt upper guide with the bolt. Ensure that the seat belt webbing is not twisted.

Tighten
Tighten the rear seat belt upper guide bolt to 52.5 N·m (39 lb ft).

5. Install the rear seat belt upper guide shoulder bolt trim cover.