For 1990-2009 cars

### Removal Procedure

1. Remove the 2 nuts securing the front legs of the rear bench seat to the floor studs.
2. Remove the 2 nuts securing the rear of the rear bench seat to the floor studs.
3. Remove the rear bench seat from the vehicle.

### Installation Procedure

1. Position the rear bench seat on the floor studs.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 2 bolts securing the rear of the bench seat to the floor studs.

Tighten
Tighten the rear bench seat mounting nuts to 52.5 N·m (39 lb ft).

3. Install the 2 nuts securing the front legs of the rear bench seat to the floor studs.

Tighten
Tighten the rear bench seat mounting nuts to 52.5 N·m (39 lb ft).