For 1990-2009 cars

### Removal Procedure

1. Remove the front hood seal. Refer to Hood Front Seal Replacement .
2. Using a grease pencil or other suitable marking device, mark the position of the hood to the hinges.
3. With the aid of an assistant, remove the 4 bolts that retain the hood to the hood hinges.
4. With the aid of an assistant, remove the hood from the vehicle.

### Installation Procedure

1. With the aid of an assistant, position the hood to the vehicle.
2. Partially install the 4 bolts that retain the hood to the hinges.

Notice: Refer to Fastener Notice in the Preface section.

3. With the aid of an assistant, position the hood to the hinges at the previously marked locations.

Tighten
Tighten the bolts to 20 N·m (15 lb ft).

4. Inspect the hood for proper adjustment. Refer to Hood Adjustment .
5. Install the front hood seal. Refer to Hood Front Seal Replacement .