For 1990-2009 cars

## Rear Seat Back Cushion Replacement Extended Cab

### Removal Procedure

1. Remove the rear seat back from the vehicle by grasping the back and lifting straight up.
2. Remove the rear seat back from the vehicle.

### Installation Procedure

1. Position the rear seat back by aligning the hooks with the slots in the vehicle.
2. Install the rear seat back by pushing the seat back downward.

## Rear Seat Back Cushion Replacement Crew Cab

### Removal Procedure

1. Release the rear seat back latches.
2. Remove the screw securing the side trim covers to the seat cushion frame.
3. Remove the bolt securing the seat back frame to the seat cushion frame.
4. Remove the seat back frame by pulling the frame off the seat cushion frame stud.
5. Inspect the white nylon bushing on the seat back frame for wear or damage and replace if necessary.

### Installation Procedure

1. Install the seat back frame by pushing the frame onto the seat cushion frame stud.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolt securing the seat back frame to the seat cushion frame.

Tighten
Tighten the seat back frame mounting bolt to 50 N·m (37 lb ft).

3. Install the screw securing the side trim covers to the seat cushion frame.