For 1990-2009 cars

### Removal Procedure

Warning: Refer to Brake Fluid Irritant Warning in the Preface section.

Caution: Refer to Brake Fluid Effects on Paint and Electrical Components Caution in the Preface section.

1. Turn the ignition switch to the OFF position.
2. Remove the brake pressure modulator valve (BPMV). Refer to Brake Pressure Modulator Valve Replacement.
3. Remove the electronic brake control module (EBCM) bolts (1).

Discard the bolts.

4. Carefully separate the EBCM (1) from the BPMV.
5. Remove the 12 EBCM to BPMV seals (2).

### Installation Procedure

1. Carefully install the EBCM (1) and the 12 seals (2) to the BPMV.

Caution: Refer to Fastener Caution in the Preface section.

Note: Do not reuse the EBCM bolts. Install new bolts.

2. Install new EBCM bolts (1) and tighten to 2 N·m (18 lb in).
3. Install the EBCM/BPMV assembly to the vehicle. Refer to Brake Pressure Modulator Valve Replacement.
4. Program the EBCM. Refer to Control Module References.