For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector (2) from the clutch pedal position switch (1).
2. Push the clutch pedal position switch retaining plate locking tabs (2) inward toward each other to release.
3. Remove the clutch pedal position switch (3) from the clutch pedal assembly (1).

### Installation Procedure

1. Slide the clutch pedal position switch (3) with retaining plate (2) into the clutch pedal bracket (1), until the locking tabs (2) are fully engaged.
2. Connect the electrical connector (2) to the clutch pedal position switch (1).
3. Complete the following in order to adjust the clutch pedal position switch (1).

3.1. | Push the switch fully into the bracket, allowing the switch to ratchet in the retaining plate.

3.2. | Depress the clutch pedal all the way to the floor.