For 1990-2009 cars

## Engine Coolant Fan Shroud Replacement LLV, LLR

### Removal Procedure

1. Remove the radiator hose-outlet. Refer to Radiator Outlet Hose Replacement .
2. Release the differential vent hose retainer.
3. Release the A/C suction hose retainer.
4. Release the A/C discharge hose retainer.
5. Rotate the slip ring counterclockwise from under the fan shroud.
6. Remove the fan shroud (3).

### Installation Procedure

1. Install the fan shroud (3) to the vehicle.
2. Rotate the slip ring to the original position.
3. Install the differential vent hose retainer.
4. Install the A/C suction hose retainer.
5. Install the A/C discharge hose retainer.
6. Install the radiator hose-outlet. Refer to Radiator Outlet Hose Replacement .

## Engine Coolant Fan Shroud Replacement LH8

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement .
3. Unclip the lower section of the shroud assembly from the upper shroud for removal.
4. Remove the radiator inlet hose. Refer to Radiator Inlet Hose Replacement .
5. Remove the radiator outlet hose retainers.
6. Remove the a/c line retainers and reposition.

1 | Fan Shroud Tab (Qty: 2)
2 | Fan Shroud