For 1990-2009 cars

## Rear Side Access Door Trim Panel Replacement Extended Cab

### Removal Procedure

1. Remove the front seat belt assembly. Refer to Front Seat Belt Replacement .
2. Remove the 2 retaining screws from the armrest.
3. Gently pull the lower side access door trim panel away from the door.
4. Remove any fasteners from the door and reinsert them in the lower side access door trim panel before installing the panel on the door.
5. Grasp the upper side access door trim panel and pull panel away from the door to release the fasteners.
6. Remove any fasteners from the door and reinsert them in the upper side access door trim panel before installing the panel on the door.

### Installation Procedure

1. Install the upper side access door trim panel to the door, ensuring that all the retaining tabs are fully seated.
2. Install the lower side access door trim panel to the door, ensuring that all the retaining tabs are fully seated.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the 2 retaining screws in the armrest.

Tighten
Tighten the rear side access door armrest screws to 2 N·m (18 lb in).

4. Install the front seat belt assembly. Refer to Front Seat Belt Replacement .