For 1990-2009 cars

Inspections | Action
--- | ---
DEFINITION: Engine continues to run after key is turned OFF, but runs very rough. If the engine runs smooth, inspect the ignition switch and the ignition switch adjustment.
Preliminary Inspections |

• | Refer to Important Preliminary Inspections Before Beginning in Symptoms - Engine Controls .

• | Search for bulletins.

• | Verify that the engine control module (ECM) grounds are clean, tight, and in the proper locations. Refer to Power and Grounding Component Views and Engine Controls Schematics .

Fuel System | Test the fuel injectors. Refer to Fuel Injector Diagnosis .