For 1990-2009 cars

### Removal Procedure

1. Remove the grille. Refer to Grille Replacement.
2. Disconnect the horn assembly electrical connector.
3. Remove the bolt that retains the horn assembly to the radiator support.
4. Remove the horn assembly from the body.

### Installation Procedure

1. Install the horn assembly to the radiator support.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolt that retains the horn assembly to the radiator support.

Tighten
Tighten the bolt to 10 N·m (88 lb in).

3. Connect the horn assembly electrical connector.
4. Install the grille. Refer to Grille Replacement.