For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Open the sunshade to the full open position.
2. Remove the sunroof front trim cover. Refer to Sunroof Front Trim Cover Replacement .
3. Remove the sunroof motor. Refer to Power Sunroof Motor Replacement .

1 | Sunroof Cam Screws (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 3 N·m (27 lb in)
2 | Sunroof Cam Plate
3 | Sunroof Cam Tip Ensure that the chamfered edge of the gear is directed upward.