For 1990-2009 cars

### Removal Procedure

1. Loosen the air cleaner outlet duct clamp (1) at the air cleaner.
2. Loosen the air cleaner outlet duct clamp (3) at the resonator.
3. Remove the air cleaner outlet duct (2).

### Installation Procedure

Note: Align the air cleaner outlet duct tab (4) to the air cleaner resonator tab (5).

1. Install the air cleaner outlet duct (2) to the resonator and the air cleaner.
2. Tighten the air cleaner outlet duct clamp (3) at the resonator.

Caution: Refer to Fastener Caution in the Preface section.

3. Tighten the air cleaner outlet duct clamp (1) at the air cleaner.

Tighten
Tighten the clamps to 6 N·m (53 lb in).