For 1990-2009 cars

#### Tools Required

• | J 38364 Steering Column Lock Plate Compressor

• | J 42137 Steering Column Lock Plate Compressor Adapter

### Removal Procedure

1. Remove the ignition lock cylinder case. Refer to Ignition Lock Cylinder Case Replacement .
2. Remove and discard the steering shaft lock plate retaining ring using compressor J 38364 and adapter J 42137 .
3. Remove the following parts from the steering column:

3.1. | The steering shaft upper bearing retainer

3.2. | The steering shaft upper bearing spring

3.3. | The steering shaft upper bearing

### Installation Procedure

1. Install the following parts onto the steering shaft assembly:

1.1. | The steering shaft upper bearing

1.2. | The steering shaft upper bearing spring

1.3. | The steering shaft upper bearing retainer

2. Install the new steering shaft lock plate retaining ring using compressor J 38364 and adapter J 42137 .

Ensure the steering shaft lock plate retaining ring is seated correctly on the steering shaft.

3. Install the ignition lock cylinder case. Refer to Ignition Lock Cylinder Case Replacement .