For 1990-2009 cars

### Removal Procedure

1. Remove the front seat belt assembly. Refer to Front Seat Belt Replacement.
2. Remove the 2 retaining screws from the armrest.
3. Gently pull the lower side access door trim panel away from the door.
4. Remove any fasteners from the door and reinsert them in the lower side access door trim panel before installing the panel on the door.
5. Grasp the upper side access door trim panel and pull panel away from the door to release the fasteners.
6. Remove any fasteners from the door and reinsert them in the upper side access door trim panel before installing the panel on the door.

### Installation Procedure

1. Install the upper side access door trim panel to the door, ensuring that all the retaining tabs are fully seated.
2. Install the lower side access door trim panel to the door, ensuring that all the retaining tabs are fully seated.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the 2 retaining screws in the armrest. Tighten the rear side access door armrest screws to 2 N·m (18 lb in).
4. Install the front seat belt assembly. Refer to Front Seat Belt Replacement.