For 1990-2009 cars

### Removal Procedure

1. Remove the lens from the dome lamp.
2. Carefully use a flat-bladed tool, and release the tabs (2) retaining to the dome lamp to the headliner.
3. Lower the dome lamp and disconnect the electrical connector (1).
4. Remove the dome lamp from the vehicle.

### Installation Procedure

1. Position the dome lamp to the headliner and connect the electrical connector (1).
2. Ensure the retaining tabs (2) are in the open position.
3. Install the dome lamp into the headliner opening and close the retaining tabs (2).
4. Ensure the dome lamp is secure to the headliner.
5. Install the lens to the dome lamp.