For 1990-2009 cars

## Rear Seat Cushion Frame Replacement Extended Cab

### Removal Procedure

1. Remove the rear folding seat cushion from the vehicle. Refer to Folding Seat Replacement.
2. Release the J-strips (2) on the cover (1).
3. Remove the seat cushion cover from the seat frame/pad.

### Installation Procedure

1. Install the seat cushion cover over the seat frame/pad.
2. Install the J-strips (2) on the cover (1).
3. Install the rear folding seat cushion in the vehicle. Refer to Folding Seat Replacement.

## Rear Seat Cushion Frame Replacement Crew Cab

### Removal Procedure

1. Remove the rear bench seat cushion from the vehicle. Refer to Rear Bench Seat Replacement .
2. Remove the rear cupholder. Refer to Rear Seat Cup Holder Replacement .
3. Remove the rear seat back assembly. Refer to Rear Seat Back Replacement .
4. Remove the rear seat cushion cover and pad. Refer to Rear Seat Cushion Cover and Pad Replacement .
5. Remove the rear seat cushion frame.

### Installation Procedure

1. Install the rear seat cushion cover and pad to the frame. Refer to Rear Seat Cushion Cover and Pad Replacement .
2. Install the rear seat back assembly. Refer to Rear Seat Back Replacement .
3. Install the rear cupholder. Refer to Rear Seat Cup Holder Replacement .
4. Install the rear bench seat cushion in the vehicle. Refer to Rear Bench Seat Replacement .