For 1990-2009 cars

### Removal Procedure

1. Remove the rear inboard seat bolt from the driver seat.
2. Remove the grommet securing the center seat belt buckle assembly (1) to the seat adjuster.
3. Remove the center seat belt buckle assembly (1).

### Installation Procedure

1. Position the seat belt buckle assembly (1) over the rear inboard seat adjuster mounting hole.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the front seat mounting bolt (2).

Tighten
Tighten the front seat mounting bolt to 52.5 N·m (39 lb ft).