For 1990-2009 cars
Master Electrical Component List
Automatic Transmission Controls Schematics
OBD II Symbol Description Notice

### Circuit Description

The 2-3 shift solenoid (SS) valve controls the fluid flow acting on the 2-3 shift valves. The 2-3 SS valve is a normally-open exhaust valve that is used with the 1-2 SS valve, in order to allow 4 different shifting combinations.

When the powertrain control module (PCM) detects a 4-3-3-4 shift pattern, then DTC P0756 sets. DTC P0756 is a type A DTC.

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC P0756 2-3 Shift Solenoid Valve Performance - No First or Second Gear

### Conditions for Running the DTC

• | No vehicle speed sensor (VSS) DTCs P0502 or P0503.

• | No 1-2 SS valve DTC P0973 or P0974.

• | No 2-3 SS valve DTC P0976 or P0977.

• | No 3-2 SS valve DTC P0787 or P0788.

• | The engine speed is greater than 475 RPM for 5 seconds.

• | The engine is not in fuel cutoff.

• | The gear range is D4, D3, D2 or D1.

• | The throttle position (TP) angle is greater than 25 percent.

• | The transmission fluid temperature is 20-130°C (68-266°F).

### Conditions for Setting the DTC

DTC P0756 sets if both of the following conditions occur:

#### Condition 1

• | The PCM commands first gear for 3 seconds.

• | The estimated gear ratio is 0 to 1.

• | The engine torque is 55-550 N·m (40-405 lb ft).

• | All conditions are met for 2 seconds.

#### Condition 2

• | The PCM commands second gear for 3 seconds.

• | The estimated gear ratio is 0.9 to 1.2.

• | The engine torque is 65-550 N·m (48-406 lb ft).

• | All conditions are met for 3 seconds.

### Action Taken When the DTC Sets

• | The PCM illuminates the malfunction indicator lamp (MIL).

• | The PCM commands third gear only.

• | The PCM commands maximum line pressure.

• | The PCM inhibits torque converter clutch (TCC) engagement.

• | The PCM freezes shift adapts from being updated.

• | The PCM records the operating conditions when the Conditions for Setting the DTC are met. The PCM stores this information as Freeze Frame and Failure Records.

• | The PCM stores DTC P0756 in PCM history.

### Conditions for Clearing the MIL/DTC

• | The PCM turns OFF the MIL during the third consecutive trip in which the diagnostic test runs and passes.

• | A scan tool can clear the MIL/DTC.

• | The PCM clears the DTC from PCM history if the vehicle completes 40 warm-up cycles without an emission-related diagnostic fault occurring.

• | The PCM cancels the DTC default actions when the fault no longer exists and/or the ignition switch is OFF long enough in order to power down the PCM.

### Diagnostic Aids

• | Verify that the transmission meets the specifications in the Shift Speed table.

• | Other internal transmission failures may cause more than one shift to occur.

• | Refer to the Shift Solenoid Valve State and Gear Ratio table.

### Test Description

The number below refers to the step number on the diagnostic table.

1. This step tests that the PCM commanded all shifts, that all shift solenoid valves responded correctly, but that all the shifts did not occur.

#### DTC P0756

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 |

1. Install a scan tool.
2. Turn ON the ignition, with the engine OFF.

Important: Before clearing the DTC, use the scan tool in order to record the Freeze Frame and Failure Records. Using the Clear Info function erases the Freeze Frame and Failure Records from the powertrain control module (PCM).

3. Record the DTC Freeze Frame and Failure Records.
4. Clear the DTC.
5. Drive the vehicle in D4 range under the following conditions:

Accelerate the vehicle, ensuring that the PCM commands 1st, 2nd, 3rd and 4th gears.

Did you detect a 4-3-3-4 shift pattern?

--

Go to Step 3

Go to Diagnostic Aids

3 |

1. Inspect the shift solenoid/hydraulic circuit for the following conditions:

• | Debris or chips in the AFL oil passage

• | Debris or chips restricting oil flow in passage #29 of the case or through the spacer plate gasket into the valve body

• | A cracked 2-3 shift solenoid

• | A 2-3 shift valve which is stuck or hung up in the valve body bore

• | A 2-3 shuttle valve which is stuck or hung up in its bore

• | Damaged seals on the shift solenoid valves -- Refer to Shift Solenoid Leak Test .

2. Clean and inspect the related valves, bores and the valve body for debris or contamination.

Did you find and correct the condition?

--

Go to Step 4

--

4 | Perform the following procedure in order to verify the repair:

1. Select DTC.
2. Select Clear Info.
3. Drive the vehicle in D4 range under the following conditions, only if traffic and road conditions permit:

Hold the throttle at 40 percent and accelerate to 64 km/h (40 mph).

4. Select Specific DTC.
5. Enter DTC P0756.

Has the test run and passed?

--

Go to Step 5

Go to Step 2

5 | With the scan tool, observe the stored information, capture info, and DTC Info. Does the scan tool display any DTCs that you have not diagnosed? | -- | Go to Diagnostic Trouble Code (DTC) List - Vehicle | System OK