For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Disconnect the engine wiring harness electrical connector from the KS (2).
3. Remove the KS retaining bolt.
4. Remove the KS (2) from the engine block.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the KS (2) and the retaining bolt to the engine block, positioning the electrical terminals down.

Tighten
Tighten the KS bolt to 25 N·m (18 lb ft).

2. Connect the engine wiring harness electrical connector to the KS (2).
3. Lower the vehicle.