For 1990-2009 cars

#### Special Tools

J 36850 Transjel Lubricant

1. Install the reaction gear support to case bearing (692) onto the internal reaction gear support (685). Retain the bearing using J 36850 transjel lubricant or equivalent.
2. Install the internal reaction gear (684) and the internal reaction gear support (685) into the case.
3. Install the reaction carrier/support thrust bearing assembly (683) into the internal reaction gear support (685). Retain bearing with J 36850 transjel lubricant .
4. Install the reaction carrier assembly (681) into the internal reaction gear.