For 1990-2009 cars

#### Tools Required

• | J 36418-1B Turbine Shaft Seal Installer

• | J 36418-2A Turbine Shaft Seal Sizer

1. Use the J 36418-1B (1) in order to install the four turbine shaft oil seal rings (619).
2. Resize oil seal rings (619) after installation:

2.1. | Place J 36418-2A (2) over the turbine shaft oil seal rings (619) and seat against input housing.

2.2. | Remove J 36418-2A (2).

2.3. | Turn J 36418-2A (2) upside down and place over the turbine shaft oil seal ring (619).

2.4. | Seat against input housing.

2.5. | Leave J 36418-2A (2) in place over the turbine shaft oil seal rings (619) until the reverse input clutch housing is installed.