For 1990-2009 cars

## Water Pump Replacement LLV,LLR

#### Tool Required

J 46406 Fan Clutch Remover and Installer

### Removal Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Remove the fan. Refer to Fan Replacement .
3. Remove the drive belt. Refer to Drive Belt Replacement or Drive Belt Replacement .
4. Using the J 46406 , secure the water pump pulley and remove the water pump pulley bolts.
5. Remove the J 46406 .
6. Remove the water pump pulley.
7. Remove the water pump bolts.
8. Remove the water pump.
9. Discard the gasket.

### Installation Procedure

1. Install a new water pump gasket.
2. Position the water pump to the engine.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the water pump bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Install the water pump pulley.
5. Install the water pump pulley bolts.
6. Using the J 46406 , secure the water pump pulley while tightening the water pump pulley bolts.

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

7. Remove the J 41240 .
8. Install the drive belt. Refer to Drive Belt Replacement or Drive Belt Replacement .
9. Install the fan. Refer to Fan Replacement .
10. Fill the cooling system with the specified coolant and concentration. Refer to Cooling System Draining and Filling .
11. Inspect for leaks.