For 1990-2009 cars

### Removal Procedure

Important: In order to minimize door realignment, do not remove both the door hinges at the same time. Replace the broken hinge first.

1. Open the front and rear side access door.
2. Clean the mounting surfaces of the hinges with a clean rag, and mark the rear door hinge locations on each surface with a grease pencil, or other suitable marker.
3. Support the rear side access door.
4. Remove the bolts retaining the hinge to the door.
5. Remove the bolts retaining the hinge to the body.
6. Remove the rear side access door hinge from the body.

### Installation Procedure

1. Position the rear side access door hinge to the alignment marks.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts retaining the hinge to the body.

Tighten
Tighten the rear side access door hinge bolts to 25 N·m (18.4 lb ft).

3. Install the bolts retaining the hinge to the door.

Tighten
Tighten the rear side access door hinge bolts to 25 N·m (18.4 lb ft).

4. Remove the support from the rear side access door.
5. Inspect the door for proper operation and alignment. Refer to Rear Door Adjustment .