For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner resonator and outlet duct. Refer to Air Cleaner Resonator and Outlet Duct Replacement.
2. Disconnect the PCV fresh air tube (6) from the air cleaner resonator (1).
3. Disconnect the PCV dirty air tube (2) from the following:

• | The camshaft cover (5)

• | The intake manifold (3)

### Installation Procedure

1. Connect the PCV fresh air tube (6) to the air cleaner resonator (1).
2. Connect the PCV dirty air tube (2) to the following:

• | The camshaft cover (5)

• | The intake manifold (3)

3. Install the air cleaner resonator and outlet duct. Refer to Air Cleaner Resonator and Outlet Duct Replacement.