For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster trim panel. Refer to Driver Knee Bolster Panel Replacement.
2. Remove the screw retaining the switch to the instrument panel (I/P).
3. Partially remove the switch from the I/P.
4. Disconnect the switch electrical connector.
5. Remove the switch from the vehicle.

### Installation Procedure

1. Position the switch to the I/P.
2. Connect the electrical connector to the switch.
3. Install the switch to the I/P.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the screw retaining the switch to the I/P.

Tighten
Tighten the screw to 2.5 N·m (22 lb in).

5. Install the knee bolster trim panel. Refer to Driver Knee Bolster Panel Replacement.