For 1990-2009 cars

## Generator Battery Control Module Replacement 4 and 5 Cylinder

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the positive and negative battery cables. Refer to Battery Positive and Negative Cable Replacement

1 | Generator Battery Control Module

#### Procedure

1. Separate the negative battery cable from the positive cable.
2. Mark the position of the generator battery control module before removing it from the battery negative cable.
3. Remove the tape and retainers holding the module in place.
4. Slide the module down the negative cable routing any additional cables through the module loop.

Tip
always use new tape and retainers when installing the generator battery control module.