For 1990-2009 cars

### Removal Procedure

1. Position the rear door window in the full up position.
2. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement.
3. Remove the rear inside door handle. Refer to Rear Side Door Inside Handle Replacement.
4. Remove the rear door speaker. Refer to Radio Rear Side Door Speaker Replacement.
5. Remove the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement.
6. Remove the bolt retaining the rear door window run channel to the inner door panel (2).
7. Slide the window run channel (1) down out of the upper window frame.
8. Remove the window run channel from the rear door.

### Installation Procedure

1. Install the window run channel to the rear door.
2. Slide the window run channel (1) up into the upper window frame.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the bolt retaining the rear door window run channel to the inner door panel (2). Tighten the rear door window run channel bolt to 9 N·m (80 lb in).
4. Install the rear door water deflector. Refer to Rear Side Door Water Deflector Replacement.
5. Install the rear door speaker. Refer to Radio Rear Side Door Speaker Replacement.
6. Install the rear inside door handle. Refer to Rear Side Door Inside Handle Replacement.
7. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement.