For 1990-2009 cars

### Removal Procedure

Caution: Refer to Brake Fluid Irritant Caution in the Preface section.

Notice: Refer to Brake Fluid Effects on Paint and Electrical Components Notice in the Preface section.

1. Remove the master cylinder assembly. Refer to Master Cylinder Replacement .
2. Remove the knee bolster trim panel. Refer to Knee Bolster Replacement .
3. Remove the retaining clip for the pushrod for the brake booster.
4. Remove the clevis pin.
5. Remove the pushrod from the brake pedal.
6. Remove the mounting nuts for the brake booster.
7. Remove the brake booster from the vehicle.

### Installation Procedure

1. Install the brake booster in the bulkhead.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the mounting nuts for the brake booster.

Tighten
Tighten the brake booster mounting nuts to 20 N·m (15 lb ft).

3. Install the pushrod on the brake pedal.
4. Install the clevis pin.
5. Install the retaining clip.
6. Adjust the stop lamp switch. Refer to Stop Lamp Switch Adjustment .
7. Adjust the cruise control release switch. Refer to Cruise Release Switch Adjustment .
8. Install the knee bolster trim panel. Refer to Knee Bolster Replacement .
9. Install the master cylinder assembly. Refer to Master Cylinder Replacement .