For 1990-2009 cars

### Removal Procedure

Caution: When removing body panels, apply tape to corners of panel and adjacent surfaces to help prevent paint damage.

Caution: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

1. Apply masking tape to protect the bumper surfaces.
2. Pry the step pad (1) from the bumper bar (2) and the reinforcement (3) using a flat-bladed plastic tool.
3. Grasp the step pad from the outer edge, pull upward to release it from the bumper bar (2) and the reinforcement (3).

### Installation Procedure

1. Position the step pad to the bumper bar (2) and the reinforcement (3).
2. Press the step pad down.
3. Remove the masking tape.