For 1990-2009 cars

### Removal Procedure

1. Remove the 2 bolts securing the rear storage compartment to the floor.
2. Remove the rear storage compartment.

### Installation Procedure

1. Position the rear storage compartment on the floor.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the 2 bolts (1) retaining the rear storage compartment to the floor. Tighten the rear storage compartment bolts to 9 N·m (79 lb in).