For 1990-2009 cars

Connector 1: | Seat Belt Buckle - Driver
Connector 2: | Seat Belt Buckle - Passenger C1
Connector 3: | Seat Belt Buckle - Passenger C2

### Seat Belt Buckle - Driver

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Buckle - Driver

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK/WH | 2151 | Low Reference
B | BK/WH | 238 | Seat Belt Switch - Left

### Seat Belt Buckle - Passenger C1

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Buckle - Passenger C1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BK/WH | 2151 | Ground
B | BK/WH | 2484 | Seat Belt Switch - Right

### Seat Belt Buckle - Passenger C2

#### Connector Part Information

- OEM: 12110293
- Service: 12117025
- Description: 3-Way F Metri-Pack 150 Series,Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Seat Belt Buckle - Passenger C2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | L-BU | 5612 | 5-Volt Reference
B | TN | 5613 | Low Reference
C | PU | 5611 | Seat Belt Tension Sensor Signal