For 1990-2009 cars

## Water Outlet Replacement With LLV and LLR

#### Tools Required

J 38185 Hose Clamp Pliers

### Removal Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Position the J 38185 to the clamp (8) in order to remove the radiator outlet hose (7) from the water outlet housing.
3. Remove the power steering pump bracket. Refer to Power Steering Pump Bracket Replacement .
4. Remove the water outlet housing bolts.
5. Remove the water outlet housing from the cylinder head.
6. Clean and inspect the water outlet housing.
7. Clean and inspect the sealing surface of the cylinder head.

### Installation Procedure

1. Position the water outlet housing to the cylinder head.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the water outlet housing bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Install the power steering pump bracket. Refer to Power Steering Pump Bracket Replacement .
4. Position the J 38185 to the clamp (8) in order to connect the radiator outlet hose (7) to the water outlet housing.
5. Fill the cooling system. Refer to Cooling System Draining and Filling .
6. Inspect all sealing surfaces for leaks after starting the engine.