For 1990-2009 cars

## Rear Seat Belt Buckle Replacement Extended Cab

### Removal Procedure

1. Remove the rear folding seat from the vehicle. Refer to Folding Seat Replacement .
2. Remove the rear seat belt buckle assembly (1) from the vehicle.

### Installation Procedure

1. Position the rear seat belt buckle assembly (1) in the vehicle under the inboard leg (2) of the rear folding seat.
2. Install the rear folding seat in the vehicle. Refer to Folding Seat Replacement .

## Rear Seat Belt Buckle Replacement Crew Cab

### Removal Procedure

1. Remove the rear bench seat from the vehicle. Refer to Rear Bench Seat Replacement.
2. Remove the grommet securing the rear seat belt buckle assembly to the seat.
3. Remove the rear seat belt buckle assembly from the seat cushion.

### Installation Procedure

1. Install the rear bench seat in the vehicle. Refer to Rear Bench Seat Replacement. Do not install the rear bench seat mounting nut.
2. Install the rear seat belt buckle through the seat cushion loop and position the seat belt buckle assembly over the rear bench seat mounting hole.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the rear bench seat mounting nut.

Tighten
Tighten the rear bench seat mounting nut to 52.5 N·m (39 lb ft).