For 1990-2009 cars

### Removal Procedure

1. Open the door.
2. Remove the screw securing the seat back release knob to the seat.
3. Remove the seat back release knob.

### Installation Procedure

1. Position the seat back release knob onto the seat assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screw securing the seat back release knob to the seat.

Tighten
Tighten the front seat back release knob screw to 1.5 N·m (13 lb in).