For 1990-2009 cars

• | Inspect the carrier connector for damaged splines and teeth. Replace as required.

• | Inspect the shift fork for wear, scoring, and damage to the thrust surfaces. Replace as required.

• | Inspect the differential sleeve and the inner output shaft for damaged splines and teeth. Replace as required.

• | Inspect the damper spring for breakage. Replace or repair the damper spring as needed.

• | Inspect the differential actuator and the engagement switch for damage and frayed wiring.