For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Inside Rearview Mirror Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

1. Remove the inside rearview mirror cover, if equipped
2. Disconnect the electrical connector, if equipped.
3. Adjust the mirror to the full upward position.
4. Loosen the set screw located at the base of the mirror.
5. Slide the mirror upward off of the rearview mirror button.
6. Refer to Control Module References for programming and setup information.

Tighten
2 N·m (18 lb in)