For 1990-2009 cars

### Removal Procedure

1. Grasp the rear door sill plate and pull the panel away from the body to release the fasteners.
2. Remove any fasteners that may have pulled away from the panel and reinstall them to the back of the panel.
3. Slide the plate inward so the plate unhooks from the door frame.
4. Remove the rear door sill plate from the vehicle.

### Installation Procedure

1. Position the rear door sill plate over the pillar and door sill.
2. Ensure that the sill plate fasteners are aligned with the holes in the body.
3. Install the sill plate by pushing firmly against the body to seat the fasteners.