For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove both of the front tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation.
3. Remove the engine protection shield if equipped. Refer to Engine Protection Shield Replacement.
4. Disconnect the outer tie rod end from the steering knuckle. Refer to Steering Linkage Outer Tie Rod Replacement.
5. Place a drain pan to catch the fluid.
6. Disconnect the power steering hose assembly from the steering gear. Refer to Power Steering Gear Inlet and Outlet Hose Replacement.
7. Remove the coupler clamp bolt from the intermediate shaft. Refer to Lower Intermediate Steering Shaft Replacement.
8. Separate the intermediate shaft from the steering gear.
9. Remove the steering gear vertical mounting nuts, the washers and the bolts.
10. Remove the steering gear horizontal mounting nuts, the washers and the bolts.
11. Remove the crossmember, 2WD ONLY. Refer to Crossmember Replacement.
12. Remove the steering gear from the vehicle.

### Installation Procedure

1. Install the steering gear into the vehicle.
2. Loose install the steering gear horizontal mounting nuts, the washers and the bolts.
3. Install the crossmember, 2WD ONLY. Refer to Crossmember Replacement.

Caution: Refer to Fastener Caution in the Preface section.

4. Loose install the steering gear vertical mounting nuts, the washers and the bolts.

• | Tighten the long bolts to 130 N·m (96 lb ft).

• | Tighten the isolator clamp bolts to 100 N·m (74 lb ft).

5. Install the intermediate shaft to the steering gear.
6. Install the coupler clamp bolt to the intermediate shaft. Refer to Lower Intermediate Steering Shaft Replacement.
7. Connect the power steering hose assembly to the steering gear. Refer to Power Steering Gear Inlet and Outlet Hose Replacement.
8. Install the engine protection shield, if equipped. Refer to Engine Protection Shield Replacement.
9. Install the outer tie rod end to the steering knuckle. Refer to Steering Linkage Outer Tie Rod Replacement.
10. Install both of the front tire and wheel assemblies. Refer to Tire and Wheel Removal and Installation.
11. Lower the vehicle.
12. Bleed the power steering system. Refer to Power Steering System Bleeding.